;Shape##OTHER##;Body material##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Ref No##OTHER##;Lighting direction##OTHER##;Dimensions L x W x H##OTHER##;Cover##OTHER##;Color temperature##OTHER##;Color##OTHER##;Control##OTHER##;Luminous flux of the fixture##OTHER##;Luminare power##OTHER##;Efficiency##OTHER##;Diffuser material##OTHER##;Power consumption##ELECTRICAL_WATTAGE##WATTS
Silver Anodized - 4000 K - 1280 lm;1/4 r 500;Aluminum, Silver Anodized;4000;1280;FNSE054-0140EB;down;524 x 524 x 88;frosted;4000 K;silver anodized;ON/OFF;1280 lm;16 W;80 lm/W;PC - 4000 K;16
Black Anodized - 4000 K - 1280 lm;1/4 r 500;Aluminum, Black Anodized;4000;1280;FNSE054-0740EB;down;524 x 524 x 88;frosted;4000 K;black anodized;ON/OFF;1280 lm;16 W;80 lm/W;PC - 4000 K;16
White Mat - 4000 K - 1280 lm;1/4 r 500;Aluminum, White Mat;4000;1280;FNSE054-1040EB;down;524 x 524 x 88;frosted;4000 K;white mat;ON/OFF;1280 lm;16 W;80 lm/W;PC - 4000 K;16
Silver Anodized - 4000 K - 1390 lm;1/4 r 500;Aluminum, Silver Anodized;4000;1390;FNSE204-0140EB;down;524 x 524 x 88;microprism;4000 K;silver anodized;ON/OFF;1390 lm;16 W;87 lm/W;PC - 4000 K;16
Black Anodized - 4000 K - 1390 lm;1/4 r 500;Aluminum, Black Anodized;4000;1390;FNSE204-0740EB;down;524 x 524 x 88;microprism;4000 K;black anodized;ON/OFF;1390 lm;16 W;87 lm/W;PC - 4000 K;16
White Mat - 4000 K - 1390 lm;1/4 r 500;Aluminum, White Mat;4000;1390;FNSE204-1040EB;down;524 x 524 x 88;microprism;4000 K;white mat;ON/OFF;1390 lm;16 W;87 lm/W;PC - 4000 K;16
Silver Anodized - 3000 K - 1230 lm;1/4 r 500;Aluminum, Silver Anodized;3000;1230;FNSE054-0130EB;down;524 x 524 x 88;frosted;3000 K;silver anodized;ON/OFF;1230 lm;16 W;77 lm/W;PC - 3000 K;16
Black Anodized - 3000 K - 1230 lm;1/4 r 500;Aluminum, Black Anodized;3000;1230;FNSE054-0730EB;down;524 x 524 x 88;frosted;3000 K;black anodized;ON/OFF;1230 lm;16 W;77 lm/W;PC - 3000 K;16
White Mat - 3000 K - 1230 lm;1/4 r 500;Aluminum, White Mat;3000;1230;FNSE054-1030EB;down;524 x 524 x 88;frosted;3000 K;white mat;ON/OFF;1230 lm;16 W;77 lm/W;PC - 3000 K;16
Silver Anodized - 3000 K - 1340 lm;1/4 r 500;Aluminum, Silver Anodized;3000;1340;FNSE204-0130EB;down;524 x 524 x 88;microprism;3000 K;silver anodized;ON/OFF;1340 lm;16 W;84 lm/W;PC - 3000 K;16
Black Anodized - 3000 K - 1340 lm;1/4 r 500;Aluminum, Black Anodized;3000;1340;FNSE204-0730EB;down;524 x 524 x 88;microprism;3000 K;black anodized;ON/OFF;1340 lm;16 W;84 lm/W;PC - 3000 K;16
White Mat - 3000 K - 1340 lm;1/4 r 500;Aluminum, White Mat;3000;1340;FNSE204-1030EB;down;524 x 524 x 88;microprism;3000 K;white mat;ON/OFF;1340 lm;16 W;84 lm/W;PC - 3000 K;16
